Mitigating harmful cyanobacterial blooms in drinking water reservoirs through *in-situ* sediment resuspension

2024-07-30

Jiao Fang1,2, Yande Li4, Ming Su1,6,\*, Tengxin Cao1,6, Xufeng Sun3, Yufan Ai1,6, Jinyi Qin5, Jianwei Yu1,6, Min Yang1,6,\*

1. State Key Laboratory of Environmental Aquatic Chemistry, Research Center for Eco-Environmental Sciences, Chinese Academy of Sciences, P.O. Box 2871, Beijing, 100085.

2. School of Environment and Spatial Informatics, China University of Mining and Technology, Xuzhou, 221116.

3. Zhejiang Weicheng Huanbao Co. Ltd., Yunxiu North Road 1200, Huzhou, 313200.

4. Management Station of Shuangxikou Reservoir, Reservoir Management Service Center of Yuyao, Ningbo, 315423.

5. School of Civil Engineering, Chang’an University, Xi’an, 710054.

6. University of Chinese Academy of Sciences, Beijing, 100049.

\* Corresponding Author: Min Yang (yangmin@rcees.ac.cn)

# Highlights

* Sediment resuspension (SR) controls algae by light reduction and TDP removal
* SR improves sediment quality by increasing ORP and inhibiting phosphorus releases
* SR technology is green and economical, can be applied in drinking water reservoirs