MIB-derived odor management based upon hydraulic regulation in small drinking water reservoirs: principle and application

2024-12-19

Jinping Lu1,4, Ming Su1,4,\*, Yuliang Su2, Jiao Fang1, Michael Burch3, Tengxin Cao1,4, Bin Wu2, Jianwei Yu1,4, Min Yang1,4,\*

1. State Key Laboratory of Environmental Aquatic Chemistry, Research Center for Eco-Environmental Sciences, Chinese Academy of Sciences, P.O. Box 2871, Beijing, 100085.

2. Zhuhai Water Environment Holdings Group Ltd., Zhuhai, 519020.

3. School of Biological Sciences, The University of Adelaide, SA, 5005.

4. University of Chinese Academy of Sciences, Beijing, 100049.

\* Corresponding Author: Min Yang ([yangmin@rcees.ac.cn](mailto:yangmin@rcees.ac.cn))

# Highlights

* 水力停留时间（HRT）增加可能会触发2-甲基异萜醇（MIB）事件。
* MIB产生的*Planktothricoides*可以通过将HRT减少到<10天来限制。
* 根据理论模型评估了14个蓝藻属的关键HRT。
* 在ZXD水库成功应用了HRT调控以控制MIB。