MIB-derived odor management based upon hydraulic regulation in small drinking water reservoirs: principle and application

2024-12-19

Jinping Lu1,4, Ming Su1,4,\*, Yuliang Su2, Jiao Fang1, Michael Burch3, Tengxin Cao1,4, Bin Wu2, Jianwei Yu1,4, Min Yang1,4,\*

1. State Key Laboratory of Environmental Aquatic Chemistry, Research Center for Eco-Environmental Sciences, Chinese Academy of Sciences, P.O. Box 2871, Beijing, 100085.

2. Zhuhai Water Environment Holdings Group Ltd., Zhuhai, 519020.

3. School of Biological Sciences, The University of Adelaide, SA, 5005.

4. University of Chinese Academy of Sciences, Beijing, 100049.

\* Corresponding Author: Min Yang (yangmin@rcees.ac.cn)

# Highlights

* Hydraulic retention time (HRT) increase can trigger 2-methylisoborneol (MIB) episodes
* MIB-producing *Planktothricoides* can be restricted by reducing HRT to <10 days
* Critical HRTs were evaluated for 14 cyanobacterial genera based on a theoretical model
* HRT regulation was successfully applied for MIB control in ZXD Reservoir